SE 4C03 Winter 2002 Specification of the Little Internet

Instructor: William M. Farmer

Revised: 11 February 2002

Computer name host1 D-Link subnet address 192.168.5.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.17 3Com subnet address 192.168.2.0 3Com subnet mask 255.255.255.0 3Com interface address 192.168.2.1

Computer name host2 D-Link subnet address 192.168.5.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.18 3Com subnet address 192.168.5.112 3Com subnet mask 255.255.255.240 3Com interface address 192.168.5.113

Computer name host3 D-Link subnet address 192.168.5.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.19 3Com subnet address 192.168.5.96 3Com subnet mask 255.255.255.240 3Com interface address 192.168.5.97

Computer name host4 D-Link subnet address 192.168.5.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.20 3Com subnet address 192.168.5.80 3Com subnet mask 255.255.255.240 3Com interface address 192.168.5.81

Computer name host5 D-Link subnet address 192.168.5.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.21 3Com subnet address 192.168.5.64 3Com subnet mask 255.255.255.240 3Com interface address 192.168.5.65

Computer name host6 D-Link subnet address 192.168.5.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.22 3Com subnet address 192.168.5.48 3Com subnet mask 255.255.255.240 3Com interface address 192.168.5.49

Computer name host7 D-Link subnet address 192.168.5.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.33 3Com subnet address 192.168.5.48 3Com subnet mask 255.255.255.240 3Com interface address 192.168.5.50

Computer name host8 D-Link subnet address 192.168.5.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.34 3Com subnet address 192.168.5.64 3Com subnet mask 255.255.255.240 3Com interface address 192.168.5.66

Computer name host9 D-Link subnet address 192.168.5.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.35 3Com subnet address 192.168.5.80 3Com subnet mask 255.255.255.240 3Com interface address 192.168.5.82

Computer name host10 D-Link subnet address 192.168.5.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.36 3Com subnet address 192.168.5.96 3Com subnet mask 255.255.255.240 3Com interface address 192.168.5.98

Computer name host11 D-Link subnet address 192.168.5.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.37 3Com subnet address 192.168.5.112 3Com subnet mask 255.255.255.240 3Com interface address 192.168.5.114

Computer name host12 D-Link subnet address 192.168.5.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.5.38 3Com subnet address 192.168.3.0 3Com subnet mask 255.255.255.0 3Com interface address 192.168.3.1

Computer name host13 D-Link subnet address 192.168.6.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.17 3Com subnet address 192.168.3.0 3Com subnet mask 255.255.255.0 3Com interface address 192.168.3.2

Computer name host14 D-Link subnet address 192.168.6.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.18 3Com subnet address 192.168.6.112 3Com subnet mask 255.255.255.240 3Com interface address 192.168.6.113

Computer name host15 D-Link subnet address 192.168.6.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.19 3Com subnet address 192.168.6.96 3Com subnet mask 255.255.255.240 3Com interface address 192.168.6.97

Computer name host16 D-Link subnet address 192.168.6.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.20 3Com subnet address 192.168.6.80 3Com subnet mask 255.255.255.240 3Com interface address 192.168.6.81

Computer name host17 D-Link subnet address 192.168.6.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.21 3Com subnet address 192.168.6.64 3Com subnet mask 255.255.255.240 3Com interface address 192.168.6.65

Computer name host18 D-Link subnet address 192.168.6.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.22 3Com subnet address 192.168.6.48 3Com subnet mask 255.255.255.240 3Com interface address 192.168.6.49

Computer name host19 D-Link subnet address 192.168.6.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.33 3Com subnet address 192.168.6.48 3Com subnet mask 255.255.255.240 3Com interface address 192.168.6.50

Computer name host20 D-Link subnet address 192.168.6.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.34 3Com subnet address 192.168.6.64 3Com subnet mask 255.255.255.240 3Com interface address 192.168.6.66

Computer name host21 D-Link subnet address 192.168.6.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.35 3Com subnet address 192.168.6.80 3Com subnet mask 255.255.255.240 3Com interface address 192.168.6.82

Computer name host22 D-Link subnet address 192.168.6.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.36 3Com subnet address 192.168.6.96 3Com subnet mask 255.255.255.240 3Com interface address 192.168.6.98

Computer name host23 D-Link subnet address 192.168.6.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.37 3Com subnet address 192.168.6.112 3Com subnet mask 255.255.255.240 3Com interface address 192.168.6.114

Computer name host24 D-Link subnet address 192.168.6.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.6.38 3Com subnet address 192.168.4.0 3Com subnet mask 255.255.255.0 3Com interface address 192.168.4.1

Computer name host25 D-Link subnet address 192.168.7.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.17 3Com subnet address 192.168.4.0 3Com subnet mask 255.255.255.0 3Com interface address 192.168.4.2

Computer name host26 D-Link subnet address 192.168.7.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.18 3Com subnet address 192.168.7.112 3Com subnet mask 255.255.255.240 3Com interface address 192.168.7.113

Computer name host27 D-Link subnet address 192.168.7.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.19 3Com subnet address 192.168.7.96 3Com subnet mask 255.255.255.240 3Com interface address 192.168.7.97

Computer name host28 D-Link subnet address 192.168.7.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.20 3Com subnet address 192.168.7.80 3Com subnet mask 255.255.255.240 3Com interface address 192.168.7.81

Computer name host29 D-Link subnet address 192.168.7.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.21 3Com subnet address 192.168.7.64 3Com subnet mask 255.255.255.240 3Com interface address 192.168.7.65

Computer name host30 D-Link subnet address 192.168.7.16 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.22 3Com subnet address 192.168.7.48 3Com subnet mask 255.255.255.240 3Com interface address 192.168.7.49

Computer name host31 D-Link subnet address 192.168.7.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.33 3Com subnet address 192.168.7.48 3Com subnet mask 255.255.255.240 3Com interface address 192.168.7.50

Computer name host32 D-Link subnet address 192.168.7.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.34 3Com subnet address 192.168.7.64 3Com subnet mask 255.255.255.240 3Com interface address 192.168.7.66

Computer name host33 D-Link subnet address 192.168.7.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.35 3Com subnet address 192.168.7.80 3Com subnet mask 255.255.255.240 3Com interface address 192.168.7.82

Computer name host34 D-Link subnet address 192.168.7.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.36 3Com subnet address 192.168.7.96 3Com subnet mask 255.255.255.240 3Com interface address 192.168.7.98

Computer name host35 D-Link subnet address 192.168.7.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.37 3Com subnet address 192.168.7.112 3Com subnet mask 255.255.255.240 3Com interface address 192.168.7.114

Computer name host36 D-Link subnet address 192.168.7.32 D-Link subnet mask 255.255.255.240 D-Link interface address 192.168.7.38 3Com subnet address 192.168.2.0 3Com subnet mask 255.255.255.0 3Com interface address 192.168.2.2